
# TC100升级教程


# TC100 Upgrade Tutorial



1. USB-C to USB-C线一端接入产品PD口，一端接入笔记本电脑USB-C口

One end of the USB-C to USB-C cable is connected to the PD port of the product, and the other end is connected to the USB-C port of the laptop


  
  
  
2.双击打开LT USB Programmer.exe 升级应用程序

Double-click to open the LT USB Programmer.exe



  
3.导入升级程序

Open the upgrade program  
  
  
  
  
4.点击GetFWVer 先读取当前版本，确定升级应用程序和电脑已存在沟通

Click "GetFWVer" to read the current version first and confirm that there is communication between the upgrade application and the laptop



5.读取到当前版本后，点击Burn升级程序

After reading the current version, click the “Burn”  
  


升级进度条100%后，提示Written successtully（设备工具编写成功） 程序升级成功

After the upgrade progress bar reaches 100%, it prompts "Written Successfully" (device tool writing is successful), indicating that the program upgrade is successful